*** TS7423L S-Parameter Data ***

------

Useful resources:
	TagoreTech Inc. https://www.tagoretech.com/

------

Matching network = 
Series transmission line, 1.8 mm, shunt capacitor, 0.2 pF at common port.
Series transmission line, 0.4 mm, shunt capacitor, 0.2 pF at RF ports.

These measurements contain matching networks.
Transmission line length from the TS7423L switch reference plane.
For examples with matching networks, please consult the TS7423L datasheet on the TagoreTech website.

------

S3P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.

RF1ON file: Useful to verify RF1 IL and RF2 ISO.
RF2ON file: Useful to verify RF2 IL and RF1 ISO.

------

For more details and additional support, please consult the TagoreTech website.
