*** TS8021N S-Parameter Data ***

------

Useful resources:
	TagoreTech Inc. https://www.tagoretech.com/

------

Matching network =
Shunt capacitor 0.3 pF at common port, 5.1 mm from edge of switch to center of cap
Shunt capacitor 0.1 pF at RF ports, 7.9 mm from edge of switch to center of cap

For examples with matching networks, please consult the TS8021N datasheet on the Tagore Technology website.

------

S5P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.

RF1ON file: Useful to verify RF1 IL and RF2 ISO.
RF2ON file: Useful to verify RF2 IL and RF1 ISO.

------

For more details and additional support, please consult the Tagore Technology website.
