*** TS8023N S-Parameter Data ***

------

Useful resources:
	TagoreTech Inc. https://www.tagoretech.com/

------

Matching network = None.
ESD High Pass Filter on Antenna Port = Pi network consisting of Shunt 120 nH inductors and two parallel 12 pF capacitors as the series elements
L: 2712SP-121_4EC 
C: 0603N120FW251

These measurements contain no matching networks.
For examples with matching networks, please consult the TS8023N datasheet on the Tagore Technology website.

------

S5P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.

RF1ON file: Useful to verify RF1 IL and RF2 ISO.
RF2ON file: Useful to verify RF2 IL and RF1 ISO.

------

For more details and additional support, please consult the TagoreTech website.
