*** TS8028N S-Parameter Data ***

------

Useful resources:
	Tagore Technology Inc. https://www.tagoretech.com/

------

Matching network = None

LT inductor is used to tune the capacitance of the TX branch, according to the desired frequency range.
With the right LT inductor, the TX isolation can be improved.
It is recommended to create the necessary matching networks after choosing the right LT inductor.
The matching components shall be soldered as close as possible to the pin of the switch TS8028N.

These measurements contain the indicated LT inductor and matching network.
For examples of how to combine the LT value with matching networks, please consult the TS8028N datasheet on the Tagore Technology website.

------

S3P file format.
	Port 1 - Common port.
	Port 2 - RF1 (RX) port.
	Port 3 - RF2 (TX) port.

RXON file: Useful to verify RX IL and TX ISO.
TXON file: Useful to verify TX IL and RX ISO.

------

For more details and additional support, please consult the Tagore Technology website.
