*** TS8029N S-Parameter Data ***

------

Useful resources:
	Tagore Technology Inc. https://www.tagoretech.com/

------

LT = 8.2 nH
Matching network = None.

LT inductor is used to tune the capacitance of the TX branch, according to the desired frequency range.
With the right LT inductor, the TX isolation can be improved.
It is recommended to create the necessary matching networks after choosing the right LT inductor.

These measurements contain only the indicated LT inductor and no matching networks.
For examples of how to combine the LT value with matching networks, please consult the TS8029N datasheet on the Tagore Technology website.

------

S3P file format.
	Port 1 - Common port.
	Port 2 - RF1 (RX) port.
	Port 3 - RF2 (TX) port.

RXON file: Useful to verify RX IL and TX ISO.
TXON file: Useful to verify TX IL and RX ISO.

------

For more details and additional support, please consult the Tagore Technology website.
