*** TS80430N S-Parameter Data ***

------

Useful resources:
	Tagore Technology Inc. https://www.tagoretech.com/

------

Matching network = 7.8 nH shunt inductor at common port.
Frequency range = 1300 MHz - 1600 MHz

The inductor shall be soldered as close as possible to the pin of the switch TS8043N at the common port.

These measurements contain the shunt inductor as matching network.
For examples with matching networks, please consult the TS80430N datasheet on the Tagore Technology website.

------

S5P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.
	Port 4 - RF3 port.
	Port 5 - RF4 port.

RF1ON file: Useful to verify RF1 IL and RF2, RF3, and RF4 ISO.
RF2ON file: Useful to verify RF2 IL and RF1, RF3, and RF4 ISO.
RF3ON file: Useful to verify RF3 IL and RF1, RF2, and RF4 ISO.
RF4ON file: Useful to verify RF4 IL and RF1, RF2, and RF3 ISO.

------

For more details and additional support, please consult the Tagore Technology website.
