*** TS8242FK S-Parameter Data ***

------

Useful resources:
	TagoreTech Inc. https://www.tagoretech.com/

------

Matching network =
Series transmission line (2.1mm), shunt capacitor 0.3 pF at the common port.
Series transmission line (1.5mm), shunt capacitor 0.2 pF at RF1 port.
Series transmission line (0.3mm), shunt capacitor 0.2 pF at RF2 port.
Series transmission line (1.5mm), shunt capacitor 0.2 pF at RF3 port.
Series transmission line (0.3mm), shunt capacitor 0.2 pF at RF4 port.

------

S5P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.
	Port 4 - RF3 port.
	Port 5 - RF4 port.

RF1ON file: Useful to verify RF1 IL and RF2, RF3, and RF4 ISO.
RF2ON file: Useful to verify RF2 IL and RF1, RF3, and RF4 ISO.
RF3ON file: Useful to verify RF3 IL and RF1, RF2, and RF4 ISO.
RF4ON file: Useful to verify RF4 IL and RF1, RF2, and RF3 ISO.

------

For more details and additional support, please consult the TagoreTech website.
