*** TS8423K S-Parameter Data ***

------

Useful resources:
	TagoreTech Inc. https://www.tagoretech.com/

------

Matching network = 
Antenna port: 0.1pF, 3.0 mm edge of switch to center of cap
RF1: 0.2 pF, 0.9 mm edge of switch to center of cap
RF2: 0.2 pF, 0.9 mm edge of switch to center of cap


For examples with matching networks, please consult the TS8329K datasheet on the Tagore Technology website.

------

S3P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.


RF1ON file: Useful to verify RF1 IL and RF2 ISO.
RF2ON file: Useful to verify RF2 IL and RF1 ISO.
ISO file: ISO/Isolation mode measurement
OFF file: VDD off mode measurement

------

For more details and additional support, please consult the TagoreTech website.