*** TS86236P S-Parameter Data ***

------

Useful resources:
	TagoreTech Inc. https://www.tagoretech.com/

------

Matching network = 18nH Shunt inductor to all RF ports (not common port).

These measurements contain matching networks.
Shunt inductors must be soldered as close as possible to the TS86236P switch reference plane.
For examples with matching networks, please consult the TS86236P datasheet on the Tagore Technology website.

------

S3P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.

RF1ON file: Useful to verify RF1 IL and RF2 ISO.
RF2ON file: Useful to verify RF2 IL and RF1 ISO.

------

For more details and additional support, please consult the Tagore Technology website.
