*** TS8242FK S-Parameter Data ***

------

Useful resources:
	TagoreTech Inc. https://www.tagoretech.com/

------

Matching network = None.

These measurements contain no matching networks.
For examples with matching networks, please consult the TS8242FK datasheet on the Tagore Technology website.

------

S5P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.
	Port 4 - RF3 port.
	Port 5 - RF4 port.

RF1ON file: Useful to verify RF1 IL and RF2, RF3, and RF4 ISO.
RF2ON file: Useful to verify RF2 IL and RF1, RF3, and RF4 ISO.
RF3ON file: Useful to verify RF3 IL and RF1, RF2, and RF4 ISO.
RF4ON file: Useful to verify RF4 IL and RF1, RF2, and RF3 ISO.

------

For more details and additional support, please consult the TagoreTech website.
